HP N19542 – 18.5V - 6.5 Amp – 120 Watt

AS358M - Low Power Dual Operational Amplifiers
Single Supply: 3V to 36V (40V Max)
[image: image1.png]M/P/G/MM Package
(SOIC-8/DIP-8/TSSOP-8/MSOP-8)

oUTPUTT o 1~ 8 O Vee

INPUT 1- 0 2 7 ED ouTPUT2

INPUT 1+ £ 3 6 FO INPUT2-
GND T 4 5 O INPUT 2+

Figure 2. Pin Configuration of AS358/358A (Top View)
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Figure 15. Battery Charger




HP N19542 – 18.5V - 6.5 Amp – 120 Watt

Cosmo K1010 Phototransistor Photocoupler (typical PTH mount)
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http://www.cosmo-ic.com/object/products/k1010.pdf
Cosmo KPC357NT (SMD mounted) - Mini-flat package General purpose Photo Coupler
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http://www.cosmo-ic.com/object/products/KPC357NT.pdf
